V-Mon Installation

If you are using the VMC-101 hardware controller, you need to install the driver before installing the V-Mon plug-in.

Follow these instructions (skip to step 4 if you are not using a VMC-101 hardware controller):
1.  Disconnect the VMC-101 from your computer.
2.  Run the setup program "vmc101_driver_setup.exe" and complete it.
3.  Connect the VMC-101 to the computer.  Windows will present a dialog to choose a driver.  It should present a choice named VMC-101.
4.  Install the V-Mon plug-in by running "Install V-Mon.exe"