**B+W 72mm Circular Polarizer with Multi-Resistant Coating**

B+W 72mm Circular Polarizer with Multi-Resistant Coating uses a rotating B+W F-Pro filter mount for added creative options. The mount has a front accessory thread and is made of brass. Compared to the earlier standard mount, the F-Pro mount, introduced in 2001, has become thinner. Now it can be used with wide angle lenses, including most 24mm focal lengths on a full frame body, without vignetting. Another advantage of the F-Pro mount is its modified retaining ring, which is no longer threaded in from the front, but holds the filter glass in place from the back. When removing a filter or lens hood that has been screwed on too tight to the filter, the retaining ring is not at risk of loosening.

**B+W 72mm Circular Polarizer with Multi-Resistant Coating-Product Features**

* F-Pro Brass Filter Mount. One advantage of the F-Pro mount is its modified retaining ring, which is no longer threaded in from the front, but holds the filter glass in place from the back.
* MRC coating. For photographers, the main advantage of MRC coating is its ability to combat flare and ghosting.

**B+W 72mm Circular Polarizer with Multi-Resistant Coating-Product Pros**

* Outstanding construction
* MRC coating to resist flare
* Great optical quality

**B+W 72mm Circular Polarizer with Multi-Resistant Coating-Product Cons**

* A bit expensive

**B+W 72mm Circular Polarizer with Multi-Resistant Coating Customer Reviews**

One of the recent customers of B+W 72mm Circular Polarizer with Multi-Resistant Coating said, “I wanted to bring out a deeper blue sky, and This filter did the trick! You get what you pay for, I'm glad I bought this one!”

B+W 72mm Circular Polarizer with Multi-Resistant Coating is a highly efficient standard circular polarizing filter for all cameras with beam splitters in the light paths of their TTL exposure meter and with autofocus lenses.